Adapter #0

==============================================================================
                    Versions
                ================
Product Name    : PERC H330 Adapter
Serial No       : 79B01WK
FW Package Build: 25.5.9.0001

                    Mfg. Data
                ================
Mfg. Date       : 09/13/17
Rework Date     : 09/13/17
Revision No     : A06
Battery FRU     : N/A

                Image Versions in Flash:
                ================
BIOS Version       : 6.33.01.0_4.19.08.00_0x06120304
Ctrl-R Version     : 5.18-0702
FW Version         : 4.300.01-8369
NVDATA Version     : 3.1511.01-0020
Boot Block Version : 3.07.00.00-0003

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Controller Id	: 0000
Vendor Id       : 1000
Device Id       : 005f
SubVendorId     : 1028
SubDeviceId     : 1f44

Host Interface  : PCIE

ChipRevision    : C0

Link Speed 	     : 3 
Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        4433221104000000 
1        4433221105000000 
2        4433221106000000 
3        4433221107000000 
4        0000000000000000 
5        0000000000000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 5d094660191f7500
BBU              : Absent
Alarm            : Absent
NVRAM            : Present
Serial Debugger  : Present
Memory           : Absent
Flash            : Present
Memory Size      : 0MB
TPM              : Absent
On board Expander: Absent
Upgrade Key      : Absent
Temperature sensor for ROC    : Present
Temperature sensor for controller    : Present

ROC temperature : 57  degree Celsius
Controller temperature : 57  degree Celcius

                Settings
                ================
Current Time                     : 12:48:42 12/1, 2024
Predictive Fail Poll Interval    : 300sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 30%
PR Rate                          : 30%
BGI Rate                         : 30%
Check Consistency Rate           : 30%
Reconstruction Rate              : 30%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 4
Delay Among Spinup Groups        : 12s
Physical Drive Coercion Mode     : 128MB
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Disabled
Ecc Bucket Size                  : 255
Ecc Bucket Leak Rate             : 240 Minutes
Restore HotSpare on Insertion    : Disabled
Expose Enclosure Devices         : Disabled
Maintain PD Fail History         : Disabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Default LD PowerSave Policy      : Controller Defined
Maximum number of direct attached drives to spin up in 1 min : 0 
Auto Enhanced Import             : No
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No
PFK in NVRAM                     : No
Use disk activity for locate     : No
POST delay			 : 90 seconds
BIOS Error Handling          	 : Pause on Errors
Current Boot Mode 		  :Normal
                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID10, RAID50, PRL 11, PRL 11 with spanning, PRL11-RLQ0 DDF layout with no span, PRL11-RLQ0 DDF layout with span
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 32 
Max Number of VDs        : 32 
Max Parallel Commands    : 240 
Max SGE Count            : 60 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 20 
Max LD per array         : 16 
Min Strip Size           : 64 KB
Max Strip Size           : 64 KB
Max Configurable CacheCade Size: 0 GB
Current Size of CacheCade      : 0 GB
Current Size of FW Cache       : 0 MB

                Device Present
                ================
Virtual Drives    : 1 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 5 
  Disks           : 4 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : Yes
Cluster Support                 : No
BBU                             : No
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : No
Snapshot Enabled                : No
Support the OCE without adding drives : Yes
Support PFK                     : No
Support PI                      : No
Support Boot Time PFK Change    : No
Disable Online PFK Change       : No
Support Shield State            : Yes
Block SSD Write Disk Cache Change: No
Support Online FW Update	: Yes

                Supported VD Operations
                ================
Read Policy          : No
Write Policy         : No
IO Policy            : No
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : Yes
Support Breakmirror  : Yes
Power Savings        : Yes

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Support Temperature                     : Yes
NCQ                                     : No
Disable Copyback                        : No
Enable JBOD                             : Yes
Enable Copyback on SMART                : No
Enable Copyback to SSD on SMART Error   : No
Enable SSD Patrol Read                  : Yes
PR Correct Unconfigured Areas           : Yes
Enable Spin Down of UnConfigured Drives : No
Disable Spin Down of hot spares         : Yes
Spin Down time                          : 30 
T10 Power State                         : Yes
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Strip Size                       : 64kB
Flush Time                       : 4 seconds
Write Policy                     : WT
Read Policy                      : None
Cache When BBU Bad               : Disabled
Cached IO                        : No
SMART Mode                       : Mode 6
Alarm Disable                    : No
Coercion Mode                    : 128MB
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : 1 
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : No
Allow SSD SAS/SATA Mix in VD     : No
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 2 
Disable Ctrl-R                   : No
Enable Web BIOS                  : No
Direct PD Mapping                : Yes
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : No
Expose Enclosure Devices         : No
Maintain PD Fail History         : No
Disable Puncturing               : No
Zero Based Enclosure Enumeration : Yes
PreBoot CLI Enabled              : No
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : No
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : Yes
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : Yes
Max LD per array                 : 16
Power Saving option              : Don't spin down unconfigured drives
Don't spin down Hot spares
Don't Auto spin down Configured Drives
Power settings apply to all drives - individual PD/LD power settings cannot be set
Max power savings option is  not allowed for LDs. Only T10 power conditions are to be used.
Cached writes are not used for spun down VDs
Can schedule disable power savings at controller level
Default spin down time in minutes: 30 
Enable JBOD                      : Yes
TTY Log In Flash                 : Yes
Auto Enhanced Import             : No
BreakMirror RAID Support         : Yes
Disable Join Mirror              : Yes
Enable Shield State              : No
Time taken to detect CME         : 60s

Exit Code: 0x00
Adapter #0

==============================================================================
                    Versions
                ================
Product Name    : PERC H330 Adapter
Serial No       : 79B01WK
FW Package Build: 25.5.9.0001

                    Mfg. Data
                ================
Mfg. Date       : 09/13/17
Rework Date     : 09/13/17
Revision No     : A06
Battery FRU     : N/A

                Image Versions in Flash:
                ================
BIOS Version       : 6.33.01.0_4.19.08.00_0x06120304
Ctrl-R Version     : 5.18-0702
FW Version         : 4.300.01-8369
NVDATA Version     : 3.1511.01-0020
Boot Block Version : 3.07.00.00-0003

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Controller Id	: 0000
Vendor Id       : 1000
Device Id       : 005f
SubVendorId     : 1028
SubDeviceId     : 1f44

Host Interface  : PCIE

ChipRevision    : C0

Link Speed 	     : 3 
Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        4433221104000000 
1        4433221105000000 
2        4433221106000000 
3        4433221107000000 
4        0000000000000000 
5        0000000000000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 5d094660191f7500
BBU              : Absent
Alarm            : Absent
NVRAM            : Present
Serial Debugger  : Present
Memory           : Absent
Flash            : Present
Memory Size      : 0MB
TPM              : Absent
On board Expander: Absent
Upgrade Key      : Absent
Temperature sensor for ROC    : Present
Temperature sensor for controller    : Present

ROC temperature : 57  degree Celsius
Controller temperature : 57  degree Celcius

                Settings
                ================
Current Time                     : 12:48:42 12/1, 2024
Predictive Fail Poll Interval    : 300sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 30%
PR Rate                          : 30%
BGI Rate                         : 30%
Check Consistency Rate           : 30%
Reconstruction Rate              : 30%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 4
Delay Among Spinup Groups        : 12s
Physical Drive Coercion Mode     : 128MB
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Disabled
Ecc Bucket Size                  : 255
Ecc Bucket Leak Rate             : 240 Minutes
Restore HotSpare on Insertion    : Disabled
Expose Enclosure Devices         : Disabled
Maintain PD Fail History         : Disabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Default LD PowerSave Policy      : Controller Defined
Maximum number of direct attached drives to spin up in 1 min : 0 
Auto Enhanced Import             : No
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No
PFK in NVRAM                     : No
Use disk activity for locate     : No
POST delay			 : 90 seconds
BIOS Error Handling          	 : Pause on Errors
Current Boot Mode 		  :Normal
                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID10, RAID50, PRL 11, PRL 11 with spanning, PRL11-RLQ0 DDF layout with no span, PRL11-RLQ0 DDF layout with span
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 32 
Max Number of VDs        : 32 
Max Parallel Commands    : 240 
Max SGE Count            : 60 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 20 
Max LD per array         : 16 
Min Strip Size           : 64 KB
Max Strip Size           : 64 KB
Max Configurable CacheCade Size: 0 GB
Current Size of CacheCade      : 0 GB
Current Size of FW Cache       : 0 MB

                Device Present
                ================
Virtual Drives    : 1 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 5 
  Disks           : 4 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : Yes
Cluster Support                 : No
BBU                             : No
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : No
Snapshot Enabled                : No
Support the OCE without adding drives : Yes
Support PFK                     : No
Support PI                      : No
Support Boot Time PFK Change    : No
Disable Online PFK Change       : No
Support Shield State            : Yes
Block SSD Write Disk Cache Change: No
Support Online FW Update	: Yes

                Supported VD Operations
                ================
Read Policy          : No
Write Policy         : No
IO Policy            : No
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : Yes
Support Breakmirror  : Yes
Power Savings        : Yes

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Support Temperature                     : Yes
NCQ                                     : No
Disable Copyback                        : No
Enable JBOD                             : Yes
Enable Copyback on SMART                : No
Enable Copyback to SSD on SMART Error   : No
Enable SSD Patrol Read                  : Yes
PR Correct Unconfigured Areas           : Yes
Enable Spin Down of UnConfigured Drives : No
Disable Spin Down of hot spares         : Yes
Spin Down time                          : 30 
T10 Power State                         : Yes
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Strip Size                       : 64kB
Flush Time                       : 4 seconds
Write Policy                     : WT
Read Policy                      : None
Cache When BBU Bad               : Disabled
Cached IO                        : No
SMART Mode                       : Mode 6
Alarm Disable                    : No
Coercion Mode                    : 128MB
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : 1 
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : No
Allow SSD SAS/SATA Mix in VD     : No
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 2 
Disable Ctrl-R                   : No
Enable Web BIOS                  : No
Direct PD Mapping                : Yes
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : No
Expose Enclosure Devices         : No
Maintain PD Fail History         : No
Disable Puncturing               : No
Zero Based Enclosure Enumeration : Yes
PreBoot CLI Enabled              : No
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : No
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : Yes
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : Yes
Max LD per array                 : 16
Power Saving option              : Don't spin down unconfigured drives
Don't spin down Hot spares
Don't Auto spin down Configured Drives
Power settings apply to all drives - individual PD/LD power settings cannot be set
Max power savings option is  not allowed for LDs. Only T10 power conditions are to be used.
Cached writes are not used for spun down VDs
Can schedule disable power savings at controller level
Default spin down time in minutes: 30 
Enable JBOD                      : Yes
TTY Log In Flash                 : Yes
Auto Enhanced Import             : No
BreakMirror RAID Support         : Yes
Disable Join Mirror              : Yes
Enable Shield State              : No
Time taken to detect CME         : 60s

Exit Code: 0x00
